# Note this requires building with IDF 4.x
CONFIG_BT_ENABLED=y
CONFIG_BTDM_CTRL_MODE_BLE_ONLY=y
CONFIG_BTDM_CTRL_MODE_BR_EDR_ONLY=
CONFIG_BTDM_CTRL_MODE_BTDM=

CONFIG_BT_NIMBLE_ENABLED=y

CONFIG_BT_NIMBLE_MAX_CONNECTIONS=4

# Pin to the same core as MP.
# Until we move to IDF 4.2+, we need NimBLE on core 0, and for synchronisation
# with the ringbuffer and scheduler MP needs to be on the same core.
# See https://github.com/micropython/micropython/issues/5489
CONFIG_BT_NIMBLE_PINNED_TO_CORE_0=y
CONFIG_BT_NIMBLE_PINNED_TO_CORE_1=n
CONFIG_BT_NIMBLE_PINNED_TO_CORE=0

# v3.3-only (renamed in 4.0)
CONFIG_BTDM_CONTROLLER_MODE_BLE_ONLY=y
CONFIG_BTDM_CONTROLLER_MODE_BR_EDR_ONLY=
CONFIG_BTDM_CONTROLLER_MODE_BTDM=
CONFIG_BLUEDROID_ENABLED=n
CONFIG_NIMBLE_ENABLED=y
CONFIG_NIMBLE_MAX_CONNECTIONS=4
CONFIG_NIMBLE_PINNED_TO_CORE_0=n
CONFIG_NIMBLE_PINNED_TO_CORE_1=y
