# For IDF >=4.2, we are able to put NimBLE on core 1, and for synchronisation
# with the ringbuffer and scheduler MP needs to be on the same core.
# MP on core 1 prevents interference with WiFi for time sensitive operations.
CONFIG_BT_NIMBLE_PINNED_TO_CORE_0=n
CONFIG_BT_NIMBLE_PINNED_TO_CORE_1=y
CONFIG_BT_NIMBLE_PINNED_TO_CORE=1
